**CONTRACTOR REGISTERED & HIGH-RISK PLANT CHECKLIST**

**If a job requires the use of any of the listed items of Registered or High-Risk Plant this checklist must be completed.**

**The Contractor must complete it and provide it to the Safety Officer.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Site:** |  | | **Contractor:** |  | | **Date:** |  |
| **Job Details:** |  | | | | | | |
| **REGISTERED PLANT** | | | | | | | |
| **Item of Plant** | **Yes**  **or**  **No** | **Item design registration number** | **Item registration number** | **Instruction manual provided for plant** | **Maintenance records are current** | **User inspections are required and recording sheets supplied** | **Confirm required Certificates or licences and currency.** |
| A packaged boiler of hazard level A, B or C to AS4343 |  |  |  |  |  |  |  |
| A tower crane |  |  |  |  |  |  |  |
| A mobile crane with a rated capacity >10 Tonnes |  |  |  |  |  |  |  |
| A boom type elevating work platform |  |  |  |  |  |  |  |
| A hoist, with a platform movement in excess 2.4 meters designed to lift people |  |  |  |  |  |  |  |
| A work box to be suspended from a crane |  |  |  |  |  |  |  |
| A pressure vessel of hazard level A, B or C to AS4343 (except gas cylinders maintained as per AS2030) |  |  |  |  |  |  |  |
| Prefabricated scaffolding |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| **HIGH RISK PLANT** | | | | | | | |
| Industrial lift trucks |  |  |  |  |  |  |  |
| Other powered mobile plant |  |  |  |  |  |  |  |
| Other specified plant as follows: |  |  |  |  |  |  |  |
| **Certificates or licences of plant operators and currency.** | **Name** |  | | **Licence Type** |  | **Expiry Date** |  |
| **Name** |  | | **Licence Type** |  | **Expiry Date** |  |
| **Name** |  | | **Licence Type** |  | **Expiry Date** |  |
| **Name** |  | | **Licence Type** |  | **Expiry Date** |  |
|  | **Name** |  | | **Licence Type** |  | **Expiry Date** |  |
| **Supervisor Name:** |  | | | | **Date:** |  | |